# Stella Integrated Debugger (a work in progress)

The debugger in Stella may never be complete, as we're constantly adding new features requested by homebrew developers. However, even in its current form it's still quite powerful, and is able to boast at least one feature that no other 2600 debugger has; it's completely cross-platform.

## Here's a (non-comprehensive) list of what the debugger can do so far:

- Display registers and memory.
- Dump state of TIA and RIOT, with things like joystick directions and NUSIZx decoded into English (more-or-less).
- Change registers/memory, including toggles for flags in P register.
- Single step/trace.
- Breakpoints - break running program and enter debugger when the Program Counter hits a predefined address; you can set as many breakpoints as you want.
- Conditional breakpoints - Break running program when some arbitrary condition is true (e.g. "breakif {a == $7f && c}" will break when the Accumulator value is $7f and the Carry flag is true, no matter where in the program this happens). Unlike the cond breaks in PCAE, Stella's are *fast*: the emulation will run at full speed unless you use lots of breakif's at the same time, or have a slow CPU.
- Watches - View contents of a location/register before every debugger prompt.
- Traps - Like breakpoints, but break on read/write/any access to *any* memory location.
- Frame advance (automatic breakpoint at beginning of next frame) You can advance multiple frames with one command.
- Supports Distella 'configuration directives', which may be used to override automatic code/data determination in the disassembly. For now, the following directives are supported: CODE, GFX, PGFX, DATA, ROW. These directives can be entered at the debugger prompt, or (automatically) loaded and saved in configuration files.
- Extensive disassembly support, both from the emulation core and with help from Distella. Where possible, the disassembly differentiates between code, player graphics and playfield graphics (ie, addresses stored in GRPx and PFx) and data (addresses used as an operand of a command). Code sections are also differentiated between actual code, and 'tentative' code (ie, areas that may represent code sections, but haven't actually been executed yet). Such tentative code is marked with a '*' symbol.
- Supports visual representation of the bitmap data of graphics areas, as well as the ability to directly edit these areas in either hex or binary.
- Support for DASM symbol files (created with DASM's -s option), including automatically loading symbol files if they're named romname.sym
- Built-in VCS.H symbols, if no symbol file is loaded.
- Symbolic names in disassembly.
- Symbolic names accepted as input.
- Tab completion for commands, symbol names and functions.
- Graphical editor for RIOT and extended RAM. Acts a lot like a spreadsheet. Input in hex, with displays for label/decimal/binary for currently-selected location.
- GUI CPU state window.
- Reset the 6502.
- Start emulator in debugger (via command-line option "-debug").
- Save CLI session to a text file.
- Supports hex, decimal, and binary input and output almost everywhere. (disassembly is still hex).
- Support for bank switching. You can see how many banks a cart has and the currently selected bank, and manually change banks.
- Registers/memory that get changed by the CPU during debugging are highlighted when they're displayed.
- Data sources for the CPU SP/A/X/Y registers, showing the resolved/source address of of load operands.
- Scanline advance (like frame advance, break at beginning of next scanline).
- TIA display is updated during step/trace, so we can see our scanlines being drawn as it happens. This isn't 100% perfect: unlike a real TIA, the one in Stella only updates when it's written to.
- Graphical TIA tab, with register names and GUI buttons for various bits (e.g. click ENAM0 to turn it on).
- GUI Disassembly window, scrollable, with checkboxes for breakpoints.
- Script (batch) file support, including auto-running a script file named after the ROM image.
- Saving the current debugger state to a script file (including breakpoints, traps, etc).
- Built-in functions for use with "breakif", to support common conditions (such as breaking when the user presses Game Select...)
- Patching ROM in-place.
- Save patched ROM ("saverom filename.bin").

## Future planned features:

- GUI for cheat codes (Cheetah and normal codes).
- Perhaps 2 panes in the disassembly window (so you can see 2 parts of the code at once).
- Add bookmark support to disassembly window.
- More "special variables" for the expression parser.
- Possibly a mini-assembler
- Possibly support for recording and playing back input files, like MAME. This isn't a debugger feature per se, but it'll make it easier to reliably trigger a bug so you can debug it.
- Various new GUI enhancements

## How to use the debugger

Pressing ` (aka backtick, backquote, grave accent) toggles the debugger on & off. When you exit the debugger, the emulation resumes at the current program counter, and continues until either a breakpoint/trap is hit, or the ` key is pressed again.

The main debugger window will look similar to the following (note that the letters here are for reference in the document below; they aren't actually present in the debugger):

For space reasons, the Prompt, TIA, I/O and Audio displays are split into 4 tabs, only one of which is visible at a time. You can use the mouse or keyboard to select which tab you want to view. Pressing Shift with the left or right arrow keys cycles between tabs from right-to-left and left-to-right, respectively. Pressing Tab cycles between widgets in the current tab (except for in the Prompt area, where 'tab' is used for something else).

You can also enter the debugger at emulator startup by giving a breakpoint on the command line:

      ; will enter the debugger the first time the instruction at "kernel" runs
      stella -break kernel mygame.bin

      ; $fffc is the 6502/6507 init vector. This command will break and enter the
      ; debugger before the first 6507 instruction runs, so you can debug the
      ; startup code:
      stella -break "*($fffc)" mygame.bin

Using the ` key will always enter the debugger at the end of the frame (scanline 262, for NTSC games). This is because Stella only checks for keystrokes once per frame. Once in the debugger, you can control execution by stepping one instruction, scanline, or frame at a time (or more than one at a time, using commands in the prompt). You can also set breakpoints or traps, which will cause the emulator to enter the debugger when they are triggered, even if it happens in mid-frame.

## Change Tracking

The debugger tracks changes to the CPU registers and RAM by displaying changed locations or registers with a red background after each step, trace, scanline, or frame advance. This sounds simple, and it is, but it's also amazingly useful.

One clarification about the change tracking: it only tracks when values have changed. If the ROM writes a value into a RAM location that already contained the same value, that's not considered a change (old value was $whatever, new value is the same, so nothing got tracked). This may change in a future version of Stella.

## (A) Prompt tab

This is a command-line interface, similar to the DOS DEBUG command or Supermon for the C=64.

Editing keys work about like you'd expect them to in Windows, but many Bash-style commands are also supported:

Home | Move cursor to beginning of line
End | Move cursor to end of line
Delete | Remove character to right of cursor
Backspace | Remove character to left of cursor
Control-a | Same function as 'Home'
Control-e | Same function as 'End'
Control-d | Same function as 'Delete'
Control-k | Remove all characters from cursor to end of line
Control-u | Remove all characters from cursor to beginning of line
Control-w | Remove entire word to left of cursor
Shift-PgUp | Scroll up through previous commands one screen/page
Shift-PgDown | Scroll down through previous commands one screen/page
Shift-Up | Scroll up through previous commands one line
Shift-Down | Scroll down through previous commands one line
Shift-Home | Scroll to beginning of commands
Shift-End | Scroll to end of commands

You can also scroll with the mouse. Copy and paste is not yet supported.

To see the available commands, enter "help". Bash-style tab completion is supported for commands, labels and functions (see below).

For now, there are some functions that only exist in the prompt. We intend to add GUI equivalents for all (or almost all?) of the prompt commands in future releases. People who like command prompts will be able to use the prompt, but people who hate them will have a fully functional debugger without typing (or without typing much, anyway).

#### Tab completion

While entering a command, label or function, you can type a partial name and press the Tab key to attempt to auto-complete it. If you've ever used "bash", this will be immediately familiar. If not, try it: load up a ROM, go to the debugger, type "print w" (but don't press Enter), then hit Tab. The "w" will change to "WSYNC" (since this is the only built-in label starting with a "w"). If there are multiple possible completions (try with "v" instead of "w"), you'll see a list of them, and your partial name will be completed as far as possible.

Tab completion works on all labels: built-in, loaded from a symbol file, or set during debugging with the "define" command. It also works with built-in functions and those defined with the "function" command, but it doesn't (yet) work on filenames.

#### Expressions

Almost every command takes a value: the "a" command takes a byte to stuff into the accumulator, the "break" command takes an address to set/clear a breakpoint at. These values can be as a hex constant ($ff, $1234), or as complex as "the low byte of the 16-bit value located at the address pointed to by the binary number 1010010110100101" (which would be "@<\1010010110100101"). You can also use registers and labels in expressions.

You can use arithmetic and boolean operators in expressions. The syntax is very C-like. The operators supported are:

          + - * /  (add, subtract, multiply, divide: 2+2 is 4)
          %        (modulus/remainder: 3%2 is 1)
          & | ^ ~  (bitwise AND, OR, XOR, NOT: 2&3 is 2)
          && || !  (logical AND, OR, NOT: 2&&3 is 1, 2||0 is 0)
          ( )      (parentheses for grouping: (2+2)*3 is 12)
          * @      (byte and word pointer dereference: *$80 is the byte stored
                    at location $80)
          [ ]      (array-style byte pointer dereference: $80[1] is the byte
                    stored at location ($80+1) or $81)
          < >      (prefix versions: low and high byte. <$abcd is $cd)
          == < > <= >= !=
                   (comparison: equality, less-than, greater-than, less-or-equals,
                    greater-or-equals, not-equals)
          << >>    (bit shifts, left and right: 1<<1 is 2, 2>>1 is 1)

Division by zero is not an error: it results in zero instead.

None of the operators change the values of their operands. There are no variable-assignment or increment/decrement operators. This may change in the future, which is why we used "==" for equality instead of just "=".

The bitwise and logical boolean operators are different in that the bitwise operators operate on all the bits of the operand (just like AND, ORA, EOR in 6502 asm), while the logical operators treat their operands as 0 for false, non-zero for true, and return either 0 or 1. So $1234&$5678 results in $1230, whereas $1234&&$5678 results in 1. This is just like C or C++...

#### Prefixes

Like some programming languages, the debugger uses prefixed characters to change the meaning of an expression. The prefixes are:

- Dereference prefixes:

  "*"
  Dereference a byte pointer. "*a" means "the byte at the address that the A register points to". If A is 255 (hex $ff), the result will be the value currently stored in memory location 255. This operator will be very familiar to you if you're a C or C++ programmer. It's equivalent to the PEEK() function in most 8-bit BASICs. Also, the debugger supports array-like byte dereferences: *address can be written as address[0]. *(address+1) can be written as address[1], etc.

  "@"
  Dereference a pointer to a word. This is just like the "*" byte deref, except it refers to a 16-bit value, occupying 2 locations, in low-byte-first format (standard for the 6507).

  The following are equivalent:

               @address
               *address+$100**(address+1)
               address[0]+#256*address[1]

  (TODO: add (indirect),y and (indirect,x) syntax)

- Hi/Lo Byte Prefixes:

  "<"
  Take the low byte of a 16-bit value. This has no effect on an 8-bit value: "a" is equal to "<a". However, "<$1234" equals "$34".

  ">"
  Take the high byte of a 16-bit value. For 8-bit values such as the Accumulator, this will always result in zero. For 16-bit values, "<$1234" = "$12".

- Number Base Prefixes:

  "#"
  Treat the input as a decimal number.

  "$"
  Treat the input as a hex number.

  "\"
  Treat the input as a binary number.

  These only have meaning when they come before a number, not a label or a register. "\1010" means 10 decimal. So do "$0a" and "#10". "a" by itself is always the Accumulator, no matter what the default base is set to.

  If you don't specify any number base prefix, the number is assumed to be in the default base. When you first start Stella, the default base is 16 (hexadecimal). You can change it with the "base" command. If you want to change the default base to decimal permanently, you can put a "base #10" command in your "autoexec.stella" file (see the section on "Startup").

  Remember, you can use arbitrarily complex expressions with any command that takes arguments (except the ones that take filenames, like "loadsym").

### Breakpoints, watches and traps, oh my!

#### Breakpoints

A breakpoint is a "hotspot" in your program that causes the emulator to stop emulating and jump into the debugger. You can set as many breakpoints as you like. The command is "break xx" where xx is any expression. If you've created a symbol file, you can use labels.

Example: you've got a label called "kernel". To break there, the command is "break kernel". After you've set the breakpoint, exit the debugger ("quit" or click the Exit button). The emulator will run until it gets to the breakpoint, then it will enter the debugger with the Program Counter pointing to the instruction at the breakpoint.

Breakpoints happen *before* an instruction is executed: the instruction at the breakpoint location will be the "next" instruction.

To remove a breakpoint, you just run the same command you used to set it. In the example, "break kernel" will remove the breakpoint. The "break" command can be thought of as a *toggle*: it turns the breakpoint on & off, like a light switch.

You could also use "clearbreaks" to remove all the breakpoints. Also, there is a "listbreaks" command that will list them all.

#### Conditional Breaks

A conditional breakpoint causes the emulator to enter the debugger when some arbitrary condition becomes true. "True" means "not zero" here: "2+2" is considered true because it's not zero. "2-2" is false, because it evaluates to zero. This is exactly how things work in C and lots of other languages, but it might take some getting used to if you've never used such a language.

Suppose you want to enter the debugger when the Game Reset switch is pressed. Looking at the Stella Programmers' Guide, we see that this switch is read at bit 0 of SWCHB. This bit will be 0 if the switch is pressed, or 1 otherwise.

To have an expression read the contents of an address, we use the dereference operator "*". Since we're looking at SWCHB, we need "*SWCHB".

We're only wanting to look at bit 0, so let's mask off all the other bits: "*SWCHB&1". The expression now evaluates to bit 0 of SWCHB. We're almost there: this will be 1 (true) if the switch is NOT pressed. We want to break if it IS pressed...

So we invert the sense of the test with a logical NOT operator (which is the "!" operator): !(*SWCHB&1). The parentheses are necessary as we want to apply the ! to the result of the &, not just the first term (the "*SWCHB").

"breakif !(*SWCHB&1)" will do the job for us. However, it's an ugly mess of letters, numbers, and punctuation. We can do a little better:

"breakif { !(*SWCHB & 1 ) }" is a lot more readable, isn't it? If you're going to use readable expressions with spaces in them, enclose the entire expression in curly braces.

Remember that Stella only checks for input once per frame, so a break condition that depends on input (like SWCHB) will always happen at the end of a frame. This is different from how a real 2600 works, but most ROMs only check for input once per frame anyway.

Conditional breaks appear in "listbreaks", numbered starting from zero. You can remove a cond-break with "delbreakif number", where the number comes from "listbreaks".

Any time the debugger is entered due to a trap, breakpoint, or conditional break, the reason will be displayed in the status area near the TIA Zoom display (area H).

#### Functions

There is one annoyance about complex expressions: once we remove the conditional break with "delbreakif" or "clearbreaks", we'd have to retype it (or search backwards with the up-arrow key) if we wanted to use it again.

We can avoid this by defining the expression as a function, then using "breakif function_name":

    	function gameReset { !(*SWCHB & 1 ) }
    	breakif gameReset

Now we have a meaningful name for the condition, so we can use it again. Not only that: we can use the function as part of a bigger expression. Suppose we've also defined a gameSelect function that evaluates to true if the Game Select switch is pressed. We want to break when the user presses both Select and Reset:

    	breakif { gameReset && gameSelect }

User-defined functions appear in "listfunctions", which shows the label and expression for each function. Functions can be removed with "delfunction label", where the labels come from "listfunctions".

If you've defined a lot of complex functions, you probably will want to re-use them in future runs of the debugger. You can save all your functions, breakpoints, conditional breaks, and watches with the "save" command. If you name your saved file the same as the ROM filename and place it in the ROM directory, it'll be auto-loaded next time you load the same ROM in Stella. The save file is just a plain text file called "rom_filename.stella", so you can edit it and add new functions, etc.

You can also create a file called "autoexec.stella" which will be loaded when the debugger starts, no matter what ROM you have loaded. The location of this file will depend on the version of Stella, as follows:

Linux/Unix | ~/.stella/autoexec.stella
Macintosh | ~/Library/Application Support/Stella/autoexec.stella
Windows | %APPDATA%\Stella\autoexec.stella OR _BASEDIR_\autoexec.stella (if a file named 'basedir.txt' exists in the application directory containing the full pathname for _BASEDIR_)

Note that these '.stella' script files are only accessed if you enter the debugger at least once during a program run. This means you can create these files, and not worry about slowing down emulation unless you're actively using the debugger.

#### Built-in Functions

Stella has some pre-defined functions for use with the "breakif" command. These allow you to break and enter the debugger on various conditions without having to define the conditions yourself.

Built-in functions and pseudo-registers always start with an _ (underscore) character. It is suggested that you don't start labels in your game's source with underscores, if you plan to use them with the Stella debugger.

Function | Definition | Description
--- | --- | ---
_joy0left | !(*SWCHA & $40) | Left joystick moved left
_joy0right | !(*SWCHA & $80) | Left joystick moved right
_joy0up | !(*SWCHA & $10) | Left joystick moved up
_joy0down | !(*SWCHA & $20) | Left joystick moved down
_joy0button | !(*INPT4 & $80) | Left joystick button pressed
_joy1left | !(*SWCHA & $04) | Right joystick moved left
_joy1right | !(*SWCHA & $08) | Right joystick moved right
_joy1up | !(*SWCHA & $01) | Right joystick moved up
_joy1down | !(*SWCHA & $02) | Right joystick moved down
_joy1button | !(*INPT5 & $80) | Right joystick button pressed
_select | !(*SWCHB & $02) | Game Select pressed
_reset | !(*SWCHB & $01) | Game Reset pressed
_color | *SWCHB & $08 | Color/BW set to Color
_bw | !(*SWCHB & $08) | Color/BW set to BW
_diff0b | !(*SWCHB & $40) | Left difficulty set to B (easy)
_diff0a | *SWCHB & $40 | Left difficulty set to A (hard)
_diff1b | !(*SWCHB & $80) | Right difficulty set to B (easy)
_diff1a | *SWCHB & $80 | Right difficulty set to A (hard)

Don't worry about memorizing them all: the Prompt "help" command will show you a list of them.

#### Pseudo-Registers

These "registers" are provided for you to use in your conditional breaks. They're not registers in the conventional sense, since they don't exist in a real system. For example, while the debugger keeps track of the number of scanlines in a frame, a real system would not (there is no register that holds 'number of scanlines' on an actual console).

Function | Description
--- | ---
_bank | Currently selected bank
_rwport | Last address to attempt a read from the cart write port
_fcount | Number of frames since emulation started
_cclocks | Color clocks on a scanline
_scan | Current scanline count
_vsync | Whether vertical sync is enabled (1 or 0)
_vblank | Whether vertical blank is enabled (1 or 0)

_scan always contains the current scanline count. You can use this to break your program in the middle of your kernel. Example:

        breakif _scan==#64

This will cause Stella to enter the debugger when the TIA reaches the beginning of the 64th scanline.

_bank always contains the currently selected bank. For 2K or 4K (non-bankswitched) ROMs, it will always contain 0. One useful use is:

        breakif { pc==myLabel && _bank==1 }

This is similar to setting a regular breakpoint, but it will only trigger when bank 1 is selected.

#### Watches

A watch is an expression that gets evaluated and printed before every prompt. This is useful for e.g. tracking the contents of a memory location while stepping through code that modifies it.

You can set up to 10 watches (in future the number will be unlimited). Since the expression isn't evaluated until it's used, you can include registers: "watch *y" will show you the contents of the location pointed to by the Y register, even if the Y register changes.

The watches are numbered. The numbers are printed along with the watches, so you can tell which is which. To delete a watch use the "delwatch" command with the watch number (1 to whatever). You can also delete them all with the "clearwatches" command.

Note that there's no real point in watching a label or CPU register without dereferencing it: Labels are constants, and CPU registers are already visible in the CPU Widget

#### Traps

A trap is similar to a breakpoint, except that it catches accesses to a memory address, rather than specific location in the program. They're useful for finding code that modifies TIA registers or memory.

An example: you are debugging a game, and you want to stop the emulation and enter the debugger whenever RESP0 is strobed. You'd use the command "trap RESP0" to set the trap, then exit the debugger. The emulator will run until the next time RESP0 is accessed (either read or write). Once the trap is hit, you can examine the TIA state to see what the actual player 0 position is, in color clocks (or you can in the future when we implement that feature in the TIA dump!)

Unlike breakpoints, traps stop the emulation *after* the instruction that triggered the trap. The reason for this is simple: until the instruction is executed, the emulator can't know it's going to hit a trap. After the trap is hit, the instruction is done executing, and whatever effects it may have had on e.g. the TIA state have already happened... but we don't have a way to run the emulated VCS in reverse, so the best we can do is stop before the next instruction runs.

Traps come in two varieties: read access traps and write access traps. It is possible to set both types of trap on the same address (that's what the plain "trap" command does). To set a read or write only trap, use "trapread" or "trapwrite". To remove a trap, you just attempt to set it again: the commands actually toggle the trap on & off. You can also get rid of all traps at once with the "cleartraps" command.

Use "listtraps" to see all enabled traps.

### Prompt commands:

Type "help" to see this list in the debugger.

                a - Set Accumulator to value xx
             bank - Show # of banks, or switch to bank xx
             base - Set default base (hex, dec, or bin)
            break - Set/clear breakpoint at address xx (default=PC)
          breakif - Set breakpoint on condition xx
                c - Carry Flag: set (0 or 1), or toggle (no arg)
            cheat - Use a cheat code (see manual for cheat types)
      clearbreaks - Clear all breakpoints
      clearconfig - Clear Distella config directives [bank xx]
       cleartraps - Clear all traps
     clearwatches - Clear all watches
              cls - Clear prompt area of text and erase history
             code - Mark 'CODE' range in disassembly
        colortest - Show value xx as TIA color
                d - Decimal Flag: set (0 or 1), or toggle (no arg)
             data - Mark 'DATA' range in disassembly
           define - Define label xx for address yy
       delbreakif - Delete conditional breakif xx
      delfunction - Delete function with label xx
         delwatch - Delete watch xx
           disasm - Disassemble address xx [yy lines] (default=PC)
             dump - Dump 128 bytes of memory at address xx
             exec - Execute script file xx
          exitrom - Exit emulator, return to ROM launcher
            frame - Advance emulation by xx frames (default=1)
         function - Define function name xx for expression yy
              gfx - Mark 'CFX' range in disassembly
             help - This cruft
             jump - Scroll disassembly to address xx
       listbreaks - List breakpoints
       listconfig - List Distella config directives [bank xx]
    listfunctions - List user-defined functions
        listtraps - List traps
       loadconfig - Load Distella config file [from file xx]
        loadstate - Load emulator state xx (0-9)
          loadsym - Load symbol file named xx
                n - Negative Flag: set (0 or 1), or toggle (no arg)
               pc - Set Program Counter to address xx
             pgfx - Mark 'PGFX' range in disassembly
            print - Evaluate/print expression xx in hex/dec/binary
              ram - Show ZP RAM, or set address xx to yy1 [yy2 ...]
            reset - Reset 6507 to init vector (excluding TIA/RIOT)
           rewind - Rewind state to last step/trace/scanline/frame
             riot - Show RIOT timer/input status
              rom - Set ROM address xx to yy1 [yy2 ...]
              row - Mark 'ROW' range in disassembly
              run - Exit debugger, return to emulator
            runto - Run until string xx in disassembly
          runtopc - Run until PC is set to value xx
                s - Set Stack Pointer to value xx
             save - Save breaks, watches, traps to file xx
       saveconfig - Save Distella config file [to file xx]
          saverom - Save (possibly patched) ROM to file xx
          saveses - Save console session to file xx
        savestate - Save emulator state xx (valid args 0-9)
         scanline - Advance emulation by xx scanlines (default=1)
             step - Single step CPU [with count xx]
              tia - Show TIA state (NOT FINISHED YET)
            trace - Single step CPU over subroutines [with count xx]
             trap - Trap read/write access to address(es) xx [to yy]
         trapread - Trap read access to address(es) xx [to yy]
        trapwrite - Trap write access to address(es) xx [to yy]
             type - Show disassembly type for address xx [to yy]
            undef - Undefine label xx (if defined)
                v - Overflow Flag: set (0 or 1), or toggle (no arg)
            watch - Print contents of address xx before every prompt
                x - Set X Register to value xx
                y - Set Y Register to value xx
                z - Zero Flag: set (0 or 1), or toggle (no arg)

## (B) TIA Tab

When selected, this tab shows detailed status of all the TIA registers (except for audio; use the Audio tab for those).

Most of the values on the TIA tab will be self-explanatory to a 2600 programmer. The top line (with all the hex values) displays the raw values read from the TIA locations, as they would be seen by the CPU.

Many of the variables inside the TIA can only be written to by the 6502. The debugger lets you get inside the TIA and see the contents of these variables. These include the color registers, player/missile graphics and positions, and the playfield.

You can control almost every aspect of the TIA from here, too: most of the displays are editable. You can even toggle individual bits in the GRP0/1 and playfield registers (remember to double-click).

The group of buttons labelled "Strobes" allows you to write to any of the strobe registers at any time.

The collision registers are displayed in decoded format, in a table. You can see exactly which objects have hit what. These are read-only displays; you can't toggle the bits in the current release of Stella. Of course, you can clear all the collisions with the CXCLR Strobe button.

To the right of each color register, you'll see a small rectangle drawn in the current color. Changing a color register will change the color of this rectangle.

## (C) I/O Tab

When selected, this tab shows detailed status of the Input, Output, and Timer portion of the RIOT/M6532 chip (the RAM portion is accessed in another part of the debugger).

As with the TIA tab, most of the values here will be self-explanatory to a 2600 programmer, and almost all can be modified. However, the SWCHx registers need further explanation:

SWCHx(W) can be modified; here, the (W) stands for write. Similarly, SWACNT/SWBCNT can be directly modified. However, the results of reading back from the SWCHx register are influenced by SWACNT/SWBCNT, and SWCHx(R) is a read-only display reflecting this result.

## (D) Audio Tab

This tab lets you view the contents of the TIA audio registers. In the current release of Stella, these are read-only displays. This tab will grow some features in a future release.

## (E) TIA Display

In the upper left of the debugger, you'll see the current frame of video as generated by the TIA. If a complete frame hasn't been drawn, the partial contents of the current frame will be displayed up to the current scanline, with the contents of the old frame (in black & white) filling the rest of the display. Note that if 'phosphor mode' has been enabled for a ROM, you will see the effect here as well. That is, no flicker will be shown for 30Hz display, even though a real system would alternate between drawing frames (and hence produce flicker).

You can use the "Scan+1" button, the prompt "scan" command, or the Alt-L key-combo to watch the TIA draw the frame one scanline at a time.

You can also right-click anywhere in this window to show a context menu, as illustrated:

The options are as follows:

- Fill to scanline: If you've already started a partial frame draw (ie, the frame is already partially 'greyed' out), selecting this option will draw all scanlines up to the vertical position where the mouse was clicked. Note that if you weren't in partial-frame mode, this option will have no effect.
- Set breakpoint: Will set a conditional breakpoint at the scanline where the mouse was clicked. Currently, you'll need to use the Prompt Tab to turn the breakpoint off again.
- Set zoom position: Influences what is shown in the TIA zoom area (further described in part (G). The zoom area will contain the area centered at the position where the mouse was clicked.
- Toggle fixed debug colors: Toggles fixed debug color mode. Note that after this is toggled, the framebuffer must be updated in some way (step/trace/frame advance) before the new colors are shown.

## (F) TIA Info

To the right of the TIA display (E) there is TIA information, as shown:

The indicators are as follows:

- Frame: The current frame number, since this ROM was loaded or reset.
- F. Cyc: The number of CPU cycles that have been executed this frame, since VSYNC was cleared at scanline 0.
- Scanline: The scanline that's currently being drawn. Scanline 0 is the one on which VSYNC is cleared (after being set for 3 scanlines, as per the Stella Programmer's Guide)
- S. Cyc: The number of CPU cycles that have been executed since the beginning of the current scanline.
- VSYNC & VBLANK: Self explanatory.
- Pixel Pos: The current number of visible color clocks that have been displayed on the current scanline, starting from the beginning of the Horizontal Blank period. During HBLANK, this value will be negative (representing the number of clocks until the first visible one). Since there are 68 color clocks per HBLANK and 160 visible clocks per scanline, the Pixel Position will range from -68 to 159.
- Color Clk: The current number of total color clocks since the beginning of this scanline's HBLANK. This counter starts at zero, but otherwise displays the same information as the Pixel Position (so Color Clock will always be 68 more than Pixel Position, and will range from 0 to 228).

## (G) TIA Zoom

Below the TIA Info (F) is the TIA Zoom area. This allows you to enlarge part of the TIA display, so you can see fine details. Note that unlike the TIA display area, this one does generate frames as the real system would. So, if you've enabled 'phosphor mode' for a ROM, it won't be honoured here (ie, you'll see alternating frames at 30Hz display, just like on a real system).

You can also right-click anywhere in this window to show a context menu, as illustrated:

These options allow you to zoom in on the image for even greater detail. If you click on the output window, you can scroll around using the cursor, PageUp/Dn and Home/End keys. You can also select the zoom position from a context menu in the TIA Display.

## (H) Breakpoint/Trap Status

Below the TIA Zoom (G), there is a status line that shows the reason the debugger was entered (if a breakpoint/trap was hit), as shown:

The output here will generally be self-explanatory. Due to space concerns, conditional breakpoints will be shown as "CBP: ...", normal breakpoints as "BP: ...", read traps as "RTrap: ..." and write traps as "WTrap: ...". See the "Breakpoints" section for details.

## (I) CPU Registers

This displays the current CPU state, as shown:

All the registers and flags are displayed, and can be changed by double-clicking on them (to the left). Flags are toggled on double-click. Selected registers here can also be changed by using the "Data Operations" buttons, further described in (J). All items are shown in hex. Any label defined for the current PC value is shown to the right. Decimal and binary equivalents are shown for SP/A/X/Y to the right (first decimal, then binary).

The column to the far right shows the 'source' of contents of the respective registers. For example, consider the command 'LDA ($80),Y'. The operand of the command resolves to some address, which isn't always easy to determine at first glance. The 'Src Addr' area shows the actual resulting operand/address being used with the given opcode.

There's not much else to say about the CPU widget: if you know 6502 assembly, it's pretty self-explanatory. If you don't, well, you should learn :)

## (J) Data Operations buttons

These buttons can be used to change values in either CPU Registers (I), or the RIOT RAM (K), depending on which of these widgets is currently active.

Each of these buttons also have a keyboard shortcut (indicated in square brackets). In fact, many of the inputboxes in various parts of the debugger respond to these same keyboard shortcuts. If in doubt, give them a try.

      0   [z]    - Set the current location/register to zero.
      Inv [i !]  - Invert the current location/register [toggle all its bits].
      Neg [n]    - Negate the current location/register [twos' complement negative].
      ++  [+ =]  - Increment the current location/register
      --  [-]    - Decrement the current location/register
      <<  [< ,]  - Shift the current location/register left.
      >>  [> .]  - Shift the current location/register right.

      Any bits shifted out of the location/register with << or >>
      are lost (they will NOT end up in the Carry flag).

## (K) M6532/RIOT and extended RAM

This is a spreadsheet-like GUI for inspecting and changing the contents of the 2600's RAM. You can view 128 bytes of RAM at a time, starting with the RAM built in to the console (zero-page RAM). If a cartridge contains extended RAM, a scrollbar will be activated, allowing to scroll in sequence through each 128 byte 'bank' of RAM. The address in the upper left corner indicates the offset (in terms of the read port) for the bank currently being displayed.

You can navigate with either the mouse or the keyboard arrow keys. To change a RAM location, either double-click on it or press Enter while it's highlighted. Enter the new value (hex only for now, sorry), then press Enter to make the change. If you change your mind, press Escape and the original value will be restored. The currently selected RAM cell can also be changed by using the Data operations buttons/associated shortcut keys (J).

Note: Many extended RAM schemes involve different addresses for reading versus writing RAM (read port vs. write port). The UI takes care of this for you; although the addresses shown are for the read port, modifying a cell will use the write port. Also, some bankswitching schemes can swap RAM and ROM dynamically during program execution. In these cases, the values shown may not always be for RAM, and may point to ROM instead. In the latter case, the data cannot be modified.

The 'Undo' button in the upper right should be self-explanatory; it will undo the most previous operation to one cell only. The 'Rev' button is more comprehensive. It will undo all operations on all cells since you first made a change.

The UI objects at the bottom refer to the currently selected RAM cell. The 'label' textbox shows the label attached to this RAM location (if any), and the other textboxes show the decimal and binary equivalent value. The remaining buttons to the right are further explained in section (L).

## (L) M6532/RIOT and extended RAM (search/compare mode)

The RAM widget also lets you search memory for values such as lives or remaining energy, but it's also very useful when debugging to determine which memory location holds which quantity.

To search RAM, click 'Srch' and enter a byte value into the search editbox (0-255). All matching values will be highlighted in the RAM widget. If 'Search' is clicked and the input is empty, all RAM locations are highlighted.

The 'Cmp' button is used to compare the given value using all addresses currently highlighted. This may be an absolute number (such as 2), or a comparitive number (such as -1). Using a '+' or '-' operator means 'search addresses for values that have changed by that amount'.

The 'Rset' button resets the entire operation; it clears the highlighted addresses and allows another search.

The following is an example of inspecting all addresses that have decreased by 1:

- Click 'Srch' with empty input. All address/values are highlighted
- Exit debugger mode and lose a life, let your energy decrease, or do whatever it is you're trying to debug
- Enter debugger mode again, click 'Cmp' and and enter a '-1' for input. This finds all values that have decreased by 1 (as compared to their current values)
- Repeatedly following these steps may help to narrow number of addresses under consideration, and eventually you'll find the memory address you're looking for
- Click 'Rset' when you're finished

## (M) ROM Listing

The ROM Widget is a disassembly of the current bank of ROM. If a symbol file is loaded, the disassembly will have labels. Even without a symbol file, the standard TIA/RIOT labels will still be present.

The disassembly is often quite extensive, and whenever possible tries to automatically differentiate between code, graphics, data and unused bytes. There are actually two levels of disassembly in Stella. First, the emulation core tracks accesses as a game is running, making for very accurate results. This is known as a dynamic analysis. Second, the built-in Distella code does a static analysis, which tentatively fills in sections that the dynamic disassembler missed (usually because the addresses haven't been accessed at runtime yet).

As such, code can be marked in two ways (absolute, when done by the emulation core), and tentative (when done by Distella, and the emulation core hasn't accessed it yet). Such 'tentative' code is marked with the '*' symbol, indicating that it has the potential to be accessed as code sometime during the program run. This gives very useful information, since it can indicate areas toggled by an option in the game (ie, when a player dies, when difficulty level changes, etc). It can also indicate whether blocks of code after a relative jump are in fact code, or simply data.

The top area contains two items:

- Current bank (x total): Shows the current bank in use (number in textbox), and the total number of banks (x). Note that bank numbers start at 0 (as in most programming languages). If the cartridge contains multiple banks, the bank can be changed in the bank textbox, and the ROM will be re-disassembled. Note that certain ROMs are quite complex, and may only show has having one 'virtual' bank when their address space can be swapped in and out in many different ways.
- Resolve data: Informs Distella about the 'resolvedata' commandline argument, which says how code and data sections are disassembled. If set to 'Never', the entire address space is treated as code. If set to 'Always', an attempt is always made to resolve data sections. The 'Automatic' setting is a combination of the previous two. First, an attempt is made to resolve data sections. If this results in the current program counter not being present in the disassembly, then a second disassembly is done, without resolving data sections. Note that this option applies only to addresses determined by Distella; addresses marked as code or graphics by the emulation core will stay as such, no matter what this setting says.

Each line of disassembly has four fields:

- Breakpoint: This is the area at the far left, to the left of the labels. Normally there will be nothing there: this indicates that there's no breakpoint set at that address. You can set and clear breakpoints by clicking in this area. When a breakpoint is set, there will be a red circle in this area. These are the same breakpoints as used by the "break" command, not the conditional "breakif" breakpoints (which makes sense: cond-breaks can break on any condition, the Program Counter isn't necessarily involved).
- Labels: Any labels assigned to the given address, either generated automatically by Distella, read from a DASM symbol file or custom labels created by the user. If 'PC addresses' is enabled, the address will be shown in grey.
- Disassembled bytes: This is either a standard 6502 mnemonic (possibly with operand), or information about graphics and/or data. For instructions, the cycle count will be included, separated by a semicolon. For graphics, a bitmap of the data, and the address of the data is included. For actual data, only the address is included.
- Hex bytes: These are the raw machine bytes for the code/graphics/data. Note that only code, graphics or data will show bytes and can be edited.

At this point, we should explain the various 'types' that the disassembler can use. These are known as 'directives', and partly correspond to configuration options from the standalone Distella program. They are listed in order of decreasing hierarchy:

CODE | Addresses which have appeared in the program counter, or which tentatively can appear in the program counter. These can be edited in hex.
GFX | Addresses which contain data stored in the player graphics registers (GRP0/GRP1). These addresses are shown with a bitmap of the graphics, which can be edited in either hex or binary. The bitmap is shown as large blocks.
PGFX | Addresses which contain data stored in the playfield graphics registers (PF0/PF1/PF2). These addresses are shown with a bitmap of the graphics, which can be edited in either hex or binary. The bitmap is shown as small dashes.
DATA | Addresses used as an operand for some opcode. These can be edited in hex.
ROW | Addresses not used as any of the above. These are shown up to 8 per line, and cannot be edited.

For code sections, the 6502 mnemonic will be UPPERCASE for all standard instructions, or lowercase for "illegal" 6502 instructions (like "dcp"). If resolving of data sections has been disabled for any reason, you'll likely see a lot of illegal opcodes if you scroll to a data table in ROM. This can also occur if the disassembler hasn't yet encountered addresses in the PC. If you step/trace/scanline/frame advance into such an area, the disassembler will make note of it, and disassemble it correctly from that point on.

You can scroll through the disassembly with the mouse or keyboard. To center the display on the current PC, press the Space bar.

Any time the Program Counter changes (due to a Step, Trace, Frame or Scanline advance, or manually setting the PC), the disassembly will scroll to the current PC location.

Even though ROM is supposed to be Read Only Memory, this is an emulator: you can change ROM all you want within the debugger. The hex bytes in the ROM Widget are editable. Double-click on them to edit them. When you're done, press Enter to accept the changes (in which case the cart will be re-disasembled) or Escape to cancel them. Note that only instructions that have been fully disassembled can be edited. In particular, blank lines or 'ROW' directives cannot be edited. If you wish to edit the latter, then the 'Resolve data' item should be set to 'Never' first. Also note that certain ROMs can have sections of address space swapped in and out dynamically. As such, changing the contents of a certain address will change the area pointed to at that time. In particular, modifying an address that points to internal RAM will change the RAM, not the underlying ROM. A future release may graphically differentiate between RAM and ROM areas.

The ROM listing also contains a context menu, accessible by right-clicking anywhere in the listing:

The following options are available:

- Save ROM: A textbox will appear for you to enter filename, and then the ROM will be saved. Note that the filename is considered relative to the current directory, not the ROM or base directory. You can enter a full path, though, in which case it doesn't matter.
- Set PC: Set the Program Counter to the address of the disassembly line where the mouse was clicked.
- RunTo PC: Single-step through code until the Program Counter matches the address of the disassembly line where the mouse was clicked.
- Toggle PC addresses: Show or hide blank labels as Program Counter addresses.
- Toggle GFX binary/hex: Switch between editing GFX and PGFX sections in either hexidecimal or binary.
- Toggle address relocation: Corresponds to the Distella '-r' option (Relocate calls out of address range).
- Re-disassemble: Self-explanatory; force the current bank to be disassembled, regardless of whether anything has changed.

### Limitations

- The ROM Widget only works on ROM or zero-page RAM separately. If your game runs code from zero-page RAM, the disassembly will show addresses $80 to $FF (zero-page RAM address space) only. Once your RAM routine returns, the ROM Widget will switch back to ROM space ($1000 - $1FFF and mirrors). The same is true of the "disasm" command; it will show either ROM or RAM space, not both at the same time.
- The standard VCS memory map has the cartridge port at locations $F000-$FFFF. However, not all the address lines exist on a 6507, so the cartridge port is "mirrored" at every other 4K chunk of address space ($1000, $3000, up to $D000). Some programmers find it easier to think of the different banks of ROM as being at different addresses (such as: Bank 0 at $D000 and bank 1 at $F000). When such a ROM runs, the Program Counter can point to one of the mirrors instead of the main area at $F000. This is perfectly OK, and everything works just fine. However, breakpoints are set on actual addresses. If there were a breakpoint set at $F010, and the bank later switched to mirror $D000, the breakpoint will not be shown, and will not break on $D010, even though it's technically the same address.

These limitations will be addressed in a future release of Stella.

## Global Buttons

There are also buttons on the right that always show up no matter which tab you're looking at. These are always active. They are: Step, Trace, Scan+1, Frame+1 and Exit. The larger button to the left (labeled '<') performs the rewind operation, which will undo the previous Step/Trace/Scan/Frame advance. The rewind buffer is currently 100 levels deep.

When you use these buttons, the prompt doesn't change. This means the status lines with the registers and disassembly will be "stale". You can update them just by re-running the relevant commands in the prompt.

You can also use the Step, Trace, Scan+1, Frame+1 and Rewind buttons from anywhere in the GUI via the keyboard, with Alt-S, Alt-T, Alt-L, Alt-F and Alt-R.

## Distella Configuration Files

As mentioned in ROM Listing (M), Stella supports the following directives: CODE/GFX/PGFX/DATA/ROW. While the debugger will try to automatically mark address space with the appropriate directive, there are times when it will fail. There are several options in this case:

1. Manually set the directives: Directives can be set in the debugger prompt with the code/gfx/pgfx/data/row commands. These accept an address range for the given directive type. Setting a range with the same type a second time will remove that directive from the range.
2. Use configuration files: Configuration files can be used to automatically load a list of directives when a ROM is loaded. These files can be generated with the 'saveconfig' command, and loaded with the 'loadconfig' command. There are also 'listconfig' and 'clearconfig' commands to show and erase (respectively) the current directive listing. Upon opening the debugger for the first time, Stella attempts to load a configuration file from several places. For this example, assume a ROM named "rr.a26", with properties entry "River Raid". Attempts will be made as follows:
   - ROM dir based on properties entry name: River Raid.cfg
   - ROM dir based on actual ROM name: rr.cfg
   - CFG dir based on properties entry name: configdir/River Raid.cfg

   The location of 'configdir' will depend on the version of Stella, as follows:

   Linux/Unix | ~/.stella/cfg/
   Macintosh | ~/Library/Application Support/Stella/cfg/
   Windows | %APPDATA%\Stella\cfg\ OR _BASEDIR_\cfg\ (if a file named 'basedir.txt' exists in the application directory containing the full pathname for _BASEDIR_)

## Tutorial: How to hack a ROM

Here is a step-by-step guide that shows you how to use the debugger to actually do something useful. No experience with debuggers is necessary, but it helps to know at least a little about 6502 programming.

1. Get the Atari Battlezone ROM image. Make sure you've got the regular NTSC version. Load it up in Stella and press TAB to get to the main menu. From there, click on "Game Information". For "Name", it should say "Battlezone (1983) (Atari)" and for MD5Sum it should say "41f252a66c6301f1e8ab3612c19bc5d4". The rest of this tutorial assumes you're using this version of the ROM; it may or may not work with the PAL version, or with any of the various "hacked" versions floating around on the 'net.
2. Start the game. You begin the game with 5 lives (count the tank symbols at the bottom of the screen).
3. Enter the debugger by pressing the ` (backquote) key. Don't get killed before you do this, though. You should still have all 5 lives.
4. In the RAM display, click the "Search" button (labelled 'Srch') and enter "5" for input. This searches RAM for your value and highlights all addresses that match the input. You should see two addresses highlighted: "00a5" and "00ba". These are the only two addresses that currently have the value 5, so they're the most likely candidates for "number of lives" counter. (However, some games might actually store one less than the real number of lives, or one more, so you might have to experiment a bit. Since this is a "rigged demo", I already know Battlezone stores the actual number of lives. Most games do, actually).
5. Exit the debugger by pressing ` (backquote) again. The game will pick up where you left off.
6. Get killed! Ram an enemy tank, or let him shoot you. Wait for the explosion to finish. You will now have 4 lives.
7. Enter the debugger again. Click the "Compare" button (labelled 'Cmp') in RAM widget and enter a value of 4. Now the RAM widget should only show one highlighted address: "00ba". What we did was search within our previous results (the ones that were 5 before) for the new value 4. Address $00ba used to have the value 5, but now it has 4. This means that Battlezone (almost certainly) stores the current number of lives at address $00ba.
8. Test your theory. Go to the RAM display and change address $ba to some high number like $ff (you could use the Prompt instead: enter "ram $ba $ff"). Exit the debugger again (or advance the frame). You should now see lots of lives at the bottom of the screen (of course, there isn't room to display $ff (255) of them!)... play the game, get killed a few times, notice that you have lots of lives.
9. Now it's time to decide what sort of "ROM hack" we want to accomplish. We've found the "lives" counter for the game, so we can either have the game start with lots of lives, or change the game code so we can't get killed (AKA immortality), or change the code so we always have the same number of lives (so we never run out, AKA infinite lives). Let's go for infinite lives: it's a little harder than just starting with lots of lives, but not as difficult as immortality (for that, we have to disable the collision checking code, which means we have to find and understand it first!)
10. Set a Write Trap on the lives counter address: "trapwrite $ba" in the Prompt. Exit the debugger and play until you get killed. When you die, the trap will cause the emulator to enter the debugger with the Program Counter pointing to the instruction *after* the one that wrote to location $ba.
11. Once in the debugger, look at the ROM display. The PC should be at address $f238, instruction "LDA $e1". You want to examine a few instructions before the PC, so scroll up using the mouse or arrow keys. Do you see the one that affects the lives counter? That's right, it's the "DEC $ba" at location $f236.
12. Let's stop the DEC $ba from happening. We can't just delete the instruction (it would mess up the addressing of everything afterwards, if it were even possible), but we can replace it with some other instruction(s).

    Since we just want to get rid of the instruction, we can replace it with NOP (no operation). From looking at the disassembly, you can see that "DEC $ba" is a 2-byte long instruction, so we will need two one-byte NOP instructions to replace it. From reading the prompt help (the "help" command), you can see that the "rom" command is what we use to patch ROM.

    Unfortunately, Stella doesn't contain an assembler, so we can't just type NOP to put a NOP instruction in the code. We'll have to use the hex opcode instead.

    Now crack open your 6502 reference manual and look up the NOP instruction's opcode... OK, OK, I'll just tell you what it is: it's $EA (234 decimal). We need two of them, so the bytes to insert will look like:

            $ea $ea

    Select the line at address $f236 and enter 'ROM patch' mode. This is done by either double-clicking the line, or pressing enter. Then delete the bytes with backspace key and enter "ea ea". Another way to do this would have been to enter "rom $f236 $ea $ea" in the Prompt widget.

13. Test your patch. First, set location $ba to some number of lives that can be displayed on the screen ("poke $ba 3" or enter directly into the RAM display). Now exit the debugger and play the game. You should see 3 lives on the screen.
14. The crucial test: get killed again! After the explosion, you will *still* see 3 lives: Success! We've hacked Battlezone to give us infinite lives.
15. Save your work. In the prompt: "saverom bzhack.bin". You now have your very own infinite-lives version of Battlezone. The file will be saved in the current directory (NOT your ROM directory), so you might want to move it to your ROM directory if it isn't the current directory. This can also be accomplished by right-clicking on the ROM widget and selecting 'Save ROM'.
16. Test the new ROM: exit Stella, and re-run it. Open your ROM (or give its name on the command line) and play the game. You can play forever! It worked.

Now, try the same techniques on some other ROM image (try Pac-Man). Some games store (lives+1) or (lives-1) instead of the actual number, so try searching for those if you can't seem to make it work.

If you successfully patch a ROM in the debugger, but the saved version won't work, or looks funny, you might need to add an entry to the stella.pro file, to tell Stella what bankswitch and/or TV type to use. That's outside the scope of this tutorial :)

Of course, the debugger is useful for a lot more than cheating and hacking ROMs. Remember, with great power comes great responsibility, so you have no excuse to avoid writing that game you've been thinking about for so long now :)