display_name = "Nintendo - SNES / Famicom (higan Accuracy)"
authors = "byuu"
supported_extensions = "sfc|smc|gb|gbc|bml|rom"
corename = "higan (Super Famicom Accuracy)"
manufacturer = "Nintendo"
categories = "Emulator"
systemname = "Super Nintendo Entertainment System"
systemid = "super_nes"
database = "Nintendo - Super Nintendo Entertainment System|Nintendo - Super Nintendo Entertainment System Hacks|Nintendo - Game Boy|Nintendo - Game Boy Color"
license = "GPLv3"
permissions = ""
display_version = "v105 (Super Famicom Accuracy)"
supports_no_game = "false"
firmware_count = 21
firmware0_desc = "dsp1.data.rom"
firmware0_path = "dsp1.data.rom"
firmware0_opt = "true"
firmware1_desc = "dsp1.program.rom"
firmware1_path = "dsp1.program.rom"
firmware1_opt = "true"
firmware2_desc = "dsp1b.data.rom"
firmware2_path = "dsp1b.data.rom"
firmware2_opt = "true"
firmware3_desc = "dsp1b.program.rom"
firmware3_path = "dsp1b.program.rom"
firmware3_opt = "true"
firmware4_desc = "dsp2.data.rom"
firmware4_path = "dsp2.data.rom"
firmware4_opt = "true"
firmware5_desc = "dsp2.program.rom"
firmware5_path = "dsp2.program.rom"
firmware5_opt = "true"
firmware6_desc = "dsp3.data.rom"
firmware6_path = "dsp3.data.rom"
firmware6_opt = "true"
firmware7_desc = "dsp3.program.rom"
firmware7_path = "dsp3.program.rom"
firmware7_opt = "true"
firmware8_desc = "dsp4.data.rom"
firmware8_path = "dsp4.data.rom"
firmware8_opt = "true"
firmware9_desc = "dsp4.program.rom"
firmware9_path = "dsp4.program.rom"
firmware9_opt = "true"
firmware10_desc = "cx4.data.rom"
firmware10_path = "cx4.data.rom"
firmware10_opt = "true"
firmware11_desc = "st010.data.rom"
firmware11_path = "st010.data.rom"
firmware11_opt = "true"
firmware12_desc = "st010.program.rom"
firmware12_path = "st010.program.rom"
firmware12_opt = "true"
firmware13_desc = "st011.data.rom"
firmware13_path = "st011.data.rom"
firmware13_opt = "true"
firmware14_desc = "st011.program.rom"
firmware14_path = "st011.program.rom"
firmware14_opt = "true"
firmware15_desc = "st018.data.rom"
firmware15_path = "st018.data.rom"
firmware15_opt = "true"
firmware16_desc = "st018.program.rom"
firmware16_path = "st018.program.rom"
firmware16_opt = "true"
firmware17_desc = "SGB1.sfc/sgb1.boot.rom (SGB Boot BIOS)"
firmware17_path = "SGB1.sfc/sgb1.boot.rom"
firmware17_opt = "true"
firmware18_desc = "SGB1.sfc/program.rom (SGB Boot Image)"
firmware18_path = "SGB1.sfc/program.rom"
firmware18_opt = "true"
firmware19_desc = "SGB2.sfc/sgb2.boot.rom (SGB Boot BIOS)"
firmware19_path = "SGB2.sfc/sgb2.boot.rom"
firmware19_opt = "true"
firmware20_desc = "SGB2.sfc/program.rom (SGB Boot Image)"
firmware20_path = "SGB2.sfc/program.rom"
firmware20_opt = "true"
notes = "[1] higan Accuracy uses split ROMS for special chip games.|[*] Notable DSP1/DSP1B Games: Super Mario Kart,  Pilotwings|[*] Notable DSP2 Games: Dungeon Master|[*] Notable DSP3 Games: SD Gundam GX|[*] Notable DSP4 Games: Top Gear 3000|[*] Notable Cx4 Games: Mega Man X2,  Mega Man X3|[2] SGB Emulation needs SGB.sfc/, SGB1.sfc/ or SGB2.sfc/ foltainers in system directory.|SGB1.sfc/ or SGB2.sfc/ can be selected as core options.|GB/GBC ROMs can be loaded directly as ROMs in this core."
